**FW upgrade instruction:**

Step 1: Printer enter update mode to update the transition file R600v03.00.00.00\_MainBT.mot

Step 2: Printer will automatically re-start and enter update mode

Step 3: To send the FW DC\_7600v10.08.03.08\_BTFWFPGA, wait for the printer to finish the update and re-start automatically.

Remark:

1. After the printer is upgraded to 10.08.03.08, it cannot downgrade to previous version (v10.08.03.07 or other old versions)

2. After the printer is upgraded to 10.08.03.08, if you want to upgrade to a new version(e.g. v10.08.03.09 or above ), it is no need to update the transition file R600v03.00.00.00\_MainBT.mot again .